|  |  |  |
| --- | --- | --- |
| Row | **Question** | **Reply** |
| 1 | The surveillance specimens are classified into three categories:  Reference Specimens (1K-3K series)  Irradiated Specimens (1Л-6Л series)  Temperature Specimens (1M-6M series)  What type of samples will be tested: Reference, Irradiated, Temperature or the first set of each category (1K, 1Л and 1M)? | All types of samples including Reference, Irradiated and Temperature specimens (first set of each category) should be tested. |
| 2 | The Reference Specimens are not irradiated.  Is it possible to perform tests of Reference specimens in ordinary accredited laboratory for destructive examinations? | It is possible to perform tests of Reference specimens in ordinary accredited laboratory for destructive examinations. |
| 3 | When the samples will be ready for testing? | The first set of all 3 categories should be withdrawn in 2019 for testing. |
| 4 | The samples (420 pieces) will be transported simultaneously or will be delivered in batches? | All samples should be transported simultaneously. |
| 5 | What are the number, dimensions and weight of the containers with specimens? | There are totally 21 containers including Reference, Irradiated and Temperature specimens.  The first set of Irradiated specimens is composed of 2 same containers by dimension of 750\*400\*200 mm with 30 kg weight. The first set of Temperature category has only one container including Temperature specimens which is a cylinder with Φ160 mm diameter and 600 mm height by 32 kg weight. |