

**ЗАО “Айкакан атомай**и**н электракаян”**

(“Армянская атомная электростанция”)

*Республика Армения, Армавирский марз, 0910, г. Мецамор*

**“Haykakan atomayin electrakayan” CJSC**

(“Armenian nuclear power plant” CJSC)

*0910, Metsamor, Armavir Region,*

*Republic of Armenia,*

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **TO/Кому:** | S. Kezin,  WANO OE Program Manager | **FROM/От:** | 1. Grigoryan,   Acting Chief Engineer of HAEK CJSC | |
|  |  |  |  | |
| **E-mail:** | Kezin@wanomc.ru | **Fax/Факс:** | 374 10 28 06 69 | |
|  |  |  |  | |
| **CC/Копия:** |  | **E-mail:** | anpp@anpp.am | |
|  |  |  |  | |
| **E-mail:** |  | **Pages/Листов:** | 1 | |
|  |  |  |  | |
| **Date/Дата:** |  | **Message/Послание No** | |  |
|  |  |  | | |
| **Subject/Тема:** | Information request for level measurement | | | |

Dear Mr. Kezin,

The Armenian NPP experiences a difficulty with level measurement in contaminated tanks (drain gully water tank, contaminated condensate tanks)

Currently a piesometer method is used at our plant for a fliud level meausurement (as to the design). The panel air supply station (БПВЩ) used for this purpose got obsolete. The spare parts are unavailable, and, as far as we know, they are not manufactured any longer.

So, in order to study existing operating experience and to fix the problem, you are kindly requested to send a request to WANO MC NPPs asking to share information on the following issues:

1. Which methods and equipment (trade mark, manufacturer) are used at your plant to measure level in contaminated tanks (vessels)?

2. In case you use the method and equipment similar to Armenian NPP, how you solve the problem with the spare parts for panel air supply station (БПВЩ)?

We are grateful in advance for provision of requested information.

A. Grigoryan Acting Chief Engineer