As mentioned in subchapter 4.2 of chapter “extreme meteorological events”, there are no independent monitoring and alerting systems for meteorological event at BNPP but warnings and meteorological conditions are sent to the BNPP through the Meteorological Centers. Two meteorological stations are Bushehr Airport and coastal meteorological stations. Meteorological information and warnings are sent to the plant via fax. Notifications are issued by the power plant crisis management.

 There are no independent records for the personnel and power plant of each incident. Other emergency documents generally originate from documents such as “personnel protection activity plan in case of accident at bushehr-1 NPP ‘related to organization of «bushehr-1» NPP
commissioning activities with document code of 52.BU.1 0.00.AB.WI.ATEX.015’ , Protecting people and the environment during the incident at unit 1 of BNPP with document code of 84.BU.10.00.GO.PLN.CMC13549 and other documents such as how to notify emergencies during the incident at the BNPP-1 with document code of 99.BU.10.0.GO.INS.CMC0044 and The Work instructions of the head of the power plant shifts ‘работы начальника смены АЭС’ with Document code of 69.BU.1 0.0.AB.RG.PD0507.

For example in chapter 4 of 52.BU.1 0.00.AB.WI.ATEX.015, the following are mentioned:

* The personnel shall act in accordance with the job descriptions, «Emergency operating instruction for reactor plant of BNPP-1» (52.BU.10.00.AB.WI.ATEX 003) and operating instructions of equipment.
* Upon receiving the forecast on anticipated impact of adverse natural factors (ANF) (earthquakes, storms, tornadoes, floods etc.), SSP shall notify the director, chief engineer, EMC members and NPP personnel about it through the communication channels. Within the period of ANF impact, the personnel shall strengthen monitoring over operation of all NPP systems and equipment. When ANF impact is over, NPP operative personnel shall perform inspection of the equipment and rooms assigned to them and report the inspection results to SSP. Sequence of «Emergency situation» announcement at Bushehr NPP and all actions of the personnel are defined in «Instruction on sequence of emergency announcement at BNPP-1 and on-line information transfer in case of radiation-hazardous situations or accidents» 99.BU.1 0.0.GO.INS.CMC0044.

 Operational procedures for plant personnel in case of accident and emergency situations are described in document with codes of 52.BU.1 0.00.AB.WI.ATEX.015.